Skip to content

# Recessed Lighting Layout: How Many Lights and Where

Spacing rules, wall offsets, beam angles and color temperature. Why professional layouts look even and DIY ones look striped.

(833) 652-8933

## Service directory — California

MAIN 200A
Emergency electrician 24/7 Electrical repair 15A Panel upgrade 200A Rewiring 12 AWG EV charger installation 50A Generator installation 22kW Lighting installation 20A Outlets and switches 20A Commercial electrical 3Ø Smart home wiring CAT6
Every circuit answered by a live dispatcher, 24 hours a day.

Lighting | Updated 2026-04-21 | Rupert Electrical Solutions

Recessed lighting is the most requested lighting job we do, and the most commonly botched. The wiring is easy. The layout is where results are won or lost, and once the holes are cut the decisions are permanent.

## Start with wall offset, not spacing

Most people begin by dividing the ceiling into a grid. That produces the classic mistake: lights centered in the room, walls in shadow, and a dark ring around the perimeter where all your artwork and cabinetry lives.

Start at the walls instead. Place the first row roughly 2 to 3 feet off the wall, which lets each fixture wash light down the vertical surface. Then space the interior fixtures evenly between those rows.

## The ceiling-height spacing rule

A workable starting point is to space fixtures at about half the ceiling height.

Ceiling height | Fixture spacing | Wall offset
--- | --- | ---
8 feet | 4 feet | 2 feet
9 feet | 4.5 feet | 2 to 2.5 feet
10 feet | 5 feet | 2.5 feet
12 feet | 6 feet | 3 feet

Tighten spacing for task areas like kitchen counters and workshops. Widen it for ambient-only spaces like a hallway or a bedroom where lamps do most of the work.

## Fixture size and beam angle

Four-inch fixtures suit hallways, accent work and tighter spacing. Six-inch fixtures are the general-purpose choice for living areas. Beam angle matters as much as size: a narrow 25 degree beam creates deliberate pools of light for accent work, while 60 degrees and wider gives the even ambient wash most rooms want. Mixing beam angles in one grid is what produces a spotty ceiling.

## Color temperature, and why the whole house should match

- 2700K warm, similar to old incandescent. Living rooms, bedrooms.
- 3000K soft white. The most versatile choice, good in kitchens and baths.
- 3500K to 4000K neutral to cool. Garages, workshops, laundry.
- 5000K+ daylight. Task-specific. In a living space it reads clinical.

Pick one temperature for connected living areas and hold it. Mixed temperatures in sightline of each other is the single most noticeable lighting error in a house, and it is instantly visible even to people who couldn't name what's wrong.

Also check the CRI. Above 90 renders skin tones and finishes accurately. Cheap fixtures at CRI 80 make a well-designed kitchen look flat and slightly grey.

## Kitchens need a different plan

The classic kitchen mistake is a symmetrical grid centered on the room. You then stand at the counter, the fixture is behind you, and you work in your own shadow.

Instead: run fixtures roughly 24 to 30 inches out from the wall so they land over the front edge of the counter rather than the backsplash. Add under-cabinet lighting, which does more for kitchen usability than any number of ceiling cans. Then treat the island separately, usually with pendants or a dedicated row.

## Dimming, and the buzzing problem

Nearly every "my new LEDs flicker" call traces to a dimmer mismatch. Older leading-edge dimmers were designed for incandescent loads and fight LED drivers. You need a dimmer rated for LED, matched to the driver type, and kept within its minimum load. Trailing-edge and ELV dimmers generally behave best.

Zone the room while you are at it. Perimeter cans, island pendants and under-cabinet lighting on separate controls is far more useful than one switch that turns everything on at full.

## Canless vs canned

Canless LED fixtures need only a small circular cut and a junction box, which makes retrofits in finished ceilings much less invasive. Traditional cans with separate trims cost more to install but let you change trims later and generally offer better optical control. For most retrofit work in existing California homes, canless is the practical answer.

## Before the first hole

Mark the full layout on the ceiling with tape and look at it for a day. Check the attic for joists, ducts, plumbing and existing cable, because a fixture 4 inches from where you want it is fine and a fixture that fights a joist is not. Confirm your circuit has capacity for the total load.

Rupert Electrical Solutions lays out every lighting installation job on the ceiling with you before cutting, statewide.

## Find an electrician in your city

We cover 482 California cities. A few of the busiest:

- Electrician in Los Angeles, CA
- Electrician in San Diego, CA
- Electrician in San Jose, CA
- Electrician in San Francisco, CA
- Electrician in Fresno, CA
- Electrician in Sacramento, CA
- Electrician in Long Beach, CA
- Electrician in Oakland, CA
- Electrician in Bakersfield, CA
- Electrician in Anaheim, CA
- Electrician in Santa Ana, CA
- Electrician in Riverside, CA
- Electrician in Stockton, CA
- Electrician in Irvine, CA
- Electrician in Chula Vista, CA
- Electrician in Fremont, CA
- Electrician in Modesto, CA
- Electrician in Oxnard, CA
- Electrician in Fontana, CA
- Electrician in Moreno Valley, CA

See all 482 cities we serve, or call (833) 652-8933 and we will confirm coverage for your address.

Previous: Power Outage Checklist for California Homeowners

Next: What an Electrical Safety Inspection Should Cover

All articles

## Book electrical work in California

Call and speak to a dispatcher now, or send the details and we will come back with a time and a price.

(833) 652-8933 Answered 24 hours a day, including holidays
Call (833) 652-8933 Request service