Skip to content

# Why Your Breaker Keeps Tripping in California (and When It's an Emergency)

A breaker that trips repeatedly is telling you something specific. Here is how California electricians read the signal, what you can safely check, and when to stop resetting and call.

(833) 652-8933

## Service directory — California

MAIN 200A
Emergency electrician 24/7 Electrical repair 15A Panel upgrade 200A Rewiring 12 AWG EV charger installation 50A Generator installation 22kW Lighting installation 20A Outlets and switches 20A Commercial electrical 3Ø Smart home wiring CAT6
Every circuit answered by a live dispatcher, 24 hours a day.

Troubleshooting | Updated 2026-01-14 | Rupert Electrical Solutions

A circuit breaker is not a nuisance device. It is a deliberately weak link, designed to fail before your wiring does. So when one trips repeatedly, the useful question is never "how do I stop it tripping" but "what is it protecting me from".

There are only three answers, and they are easy to tell apart once you know what to look for.

## 1. Overload: too much current on one circuit

A 15 amp circuit carries about 1,800 watts. A 20 amp circuit carries about 2,400. Run a 1,500 watt space heater and a 1,200 watt kettle on the same bedroom circuit and it will trip, every time, and there is nothing wrong with your wiring.

The signature of an overload is predictability. It trips when you use the same combination of things, and it takes anything from a few seconds to a few minutes to go. Unplug something and it holds.

The correct fix is not a bigger breaker. Putting a 20 amp breaker on 14 gauge wire means the wire now overheats before the breaker trips, which is exactly the failure the breaker existed to prevent. The fix is a outlet & switch installation for the heavy appliance, or more capacity through an electrical panel upgrade.

## 2. Short circuit: hot touching neutral or ground

A short trips the breaker instantly and often with a bang. Reset it and it goes again the moment you push the handle, with no load connected at all.

Common causes are a nail or screw driven through a cable during a remodel, a damaged extension cord, rodent damage in an attic, or water in an exterior box. This is not a wait-until-Monday problem, because the fault point is dumping enormous current into whatever it is touching. Leave the breaker off and call an 24/7 emergency electrician.

## 3. Ground fault or arc fault: the protection is doing its job

If a GFCI outlet or breaker trips, current is leaking somewhere it shouldn't, often through moisture. Bathroom and outdoor circuits do this after rain. An AFCI breaker, required in bedrooms and living areas, trips on the electrical signature of arcing, which is the actual mechanism behind most electrical fires in walls.

People assume a nuisance-tripping AFCI is a faulty breaker. Sometimes it is. More often it is a loose back-stabbed receptacle connection arcing under load, which is precisely what the device was installed to catch.

## What you can safely check yourself

- Unplug everything on the circuit, then reset. If it holds, add loads back one at a time. You have found an overload or a bad appliance.
- Look for a tripped GFCI upstream. One GFCI can protect an entire run of outlets, and the reset button is often in a garage or bathroom two rooms away.
- Check outdoor covers after rain. Water in an in-use cover is a very common seasonal ground fault across California.

## When to stop and call

Stop resetting and pick up the phone if any of these apply. Repeated resetting of a faulting circuit heats the breaker contacts and the fault point, and it is how a bad connection becomes a wall fire.

- The breaker trips instantly with nothing plugged in.
- Anything smells hot, sharp or like burning plastic.
- The breaker or panel cover is warm to the touch.
- You see scorch marks, discoloration or melted plastic at an outlet or in the panel.
- The breaker will not reset at all, or the handle feels loose and springy.
- It is a Zinsco or Federal Pacific panel. Those breakers have a documented history of failing to trip when they should.

## The diagnostic order a good electrician follows

There is a sequence to this, and skipping it is why some companies replace three parts and still don't fix the problem. Meter the circuit under load. Isolate by splitting the run in half and testing each leg. Inspect every device and box on the faulting leg, because loose terminations account for the majority of what we find. Only then replace the breaker, and only if the breaker itself tested bad.

Rupert Electrical Solutions runs that sequence on every electrical repair call, statewide, and we tell you what failed rather than just handing over an invoice.

## Find an electrician in your city

We cover 482 California cities. A few of the busiest:

- Electrician in Los Angeles, CA
- Electrician in San Diego, CA
- Electrician in San Jose, CA
- Electrician in San Francisco, CA
- Electrician in Fresno, CA
- Electrician in Sacramento, CA
- Electrician in Long Beach, CA
- Electrician in Oakland, CA
- Electrician in Bakersfield, CA
- Electrician in Anaheim, CA
- Electrician in Santa Ana, CA
- Electrician in Riverside, CA
- Electrician in Stockton, CA
- Electrician in Irvine, CA
- Electrician in Chula Vista, CA
- Electrician in Fremont, CA
- Electrician in Modesto, CA
- Electrician in Oxnard, CA
- Electrician in Fontana, CA
- Electrician in Moreno Valley, CA

See all 482 cities we serve, or call (833) 652-8933 and we will confirm coverage for your address.

Next: Electrical Panel Upgrade Cost in California: What Actually Drives the Price

All articles

## Book electrical work in California

Call and speak to a dispatcher now, or send the details and we will come back with a time and a price.

(833) 652-8933 Answered 24 hours a day, including holidays
Call (833) 652-8933 Request service